# Bridge Flow Ratio Calibration
Needs: | Flow | Temperature

You need to do the bed level calibration and the filament flow calibration before this one. It's better if you have done the filament temperature calibration as well.

This test will print test samples with various levels of bridge flow ratio. It starts at your current setting, so you may want to set them to 100% before clicking on the button.

## Notes

This test set the setting "Complete individual objects" to true, so you may want to reset your print settings afterwards, or disable this setting if your bed is too small.

Licence for models used for this calibration test: CC BY-SA 3.0